|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **RAIN GARDEN MAINTENANCE & INSPECTION CHECKLIST** | | | | | | |
| Payne Park, City of Pawtucket  Site name:  Inspector:  Date:  Start/Finish Time: to | |  | | |  | |
| **GENERAL MAINTENANCE & INSPECTION ITEMS** | **N/A** | **DONE** | **NEEDS REPAIR** | **COMMENTS** | | |
| For first 3 years, water **ALL** new trees weekly so that soil to depth of roots is moist. |  |  |  |  | | |
| Mow turf and direct cuttings away from gardens. |  |  |  |  | | |
| Weed-whack around inlet and outlet structures (boulders). |  |  |  |  | | |
| Remove trash and debris from within and around gardens. |  |  |  |  | | |
| Access flow channels and clear out debris, trash and sediment. |  |  |  |  | | |
| Remove weedy and invasive plants. |  |  |  |  | | |
| Remove sediment build-up, especially at inlets & outlets.\* |  |  |  |  | | |
| Remove and replace any dead plugs with approved plants. |  |  |  |  | | |
| Repair soil erosion gullies throughout rain garden, around inflow & outflow areas. |  |  |  |  | | |
| Repair erosion on all contributing areas within park. |  |  |  |  | | |
| Fill in animal burrows within or near rain gardens. |  |  |  |  | | |
| Repair signage if faded, or tagged, and replace if missing. |  |  |  |  | | |
| Comments: | | | | | |  |

*\* Sediment shall be disposed of offsite in a pre-approved location*

August 2018

**EXAMPLE**

Prepared by City of Pawtucket, designer Tim Gerrish, of Gardner&Gerrish Landscape Architects LLC, and, with funding from Rhode Island Department of Transportation, URI Cooperative Extension. These editable templates are intended for use by municipalities, designers, and others to customize for their own projects.